{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":14,"n_cols":3,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["MSE Wall Backfill Quantities:"]
["From Corridor Modeler Report\n(US 218 Sta. 241471+22.39 to\nSta. 241474+45.72):",7965.41,"CY"]
[]
["Calculated\n(US 218 Sta. 241474+45.72 to \nSta. 241474+51.72):",{"$f":"ROUND((24147451.72-24147445.72)*47.5*(937.52-0.5-917)/27,2)","v":211.32},"CY"]
[]
[null,{"$f":"SUM(B2:B4)","v":8176.73},"CY"]
[]
[]
["MSE Wall Surface Area Quantities:"]
["East Face (Wall Sta. 1001+77.39 to\nSta. 1002+52.39)",1539.6364000000001,"SF"]
["North Face (Wall Sta. 1002+52.39 to\nSta. 1003+01.22)",1001.9915999999999,"SF"]
["West Face (Wall Sta. 1003+01.22 to\nSta. 1006+31.22)",7396.0573999999997,"SF"]
[]
[null,{"$f":"SUM(B10:B13)","v":9937.6854000000003},"SF"]